**Rapport d'analyse CEM - Données traitées**

|  |  |  |  |
| --- | --- | --- | --- |
| **Sample ID:** | CRE2-2025-TP002-01 | **Configuration:** | Configuration (Mode 3) RBW 9kHz |
| **Date de traitement:** | 20/09/2025 | **Verdict global:** | FAIL |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Section** | **Frequency (MHz)** | **Polarization** | **Measure (dBµV/m)** | **Limit (dBµV/m)** | **Margin (dB)** | **Verdict** |
| 9kHz | 1.26775 | Vertical | - | RNDS-C-00517 V4.0 | 30 | PASS |
| GNSS | 1175.91025 | Vertical | - | RNDS-C-00517 V4.0 | 5 | PASS |
| GNSS | 1175.91025 | Vertical | - | Horizontal | 4 | PASS |
| GNSS | 1175.9125 | Vertical | - | Horizontal | 4 | PASS |
| GNSS | 1175.91025 | Vertical | - | Horizontal | 1 | PASS |
| 120kHz | 432.02 | Vertical | - | RNDS-C-00517 V4.0 | 4 | PASS |
| Q-Peak | 432.56 | Vertical | - | - | 2 | **FAIL** |
| Q-Peak | 433.49 | Vertical | - | - | 4 | **FAIL** |
| Q-Peak | 432.5 | Vertical | - | - |  | **FAIL** |
| 1MHz | 239 | Vertical | 4 | RNDS-C-00517 V4.0 |  | **FAIL** |
| Peak | 244.25 | Vertical | 12 | - |  | **FAIL** |
| Peak | 239.25 | Vertical | 12 | - |  | **FAIL** |
| Peak | 242.5 | Vertical | 10 | - |  | **FAIL** |
| 9kHz | 1.25875 | Vertical | - | RNDS-C-00517 V4.0 | 30 | PASS |
| GNSS | 1175.91025 | Vertical | - | RNDS-C-00517 V4.0 |  | PASS |
| GNSS | 1175.908 | Vertical | - | Horizontal | 1 | PASS |
| GNSS | 1175.908 | Vertical | - | Horizontal |  | **FAIL** |
| GNSS | 1175.908 | Vertical | 6 | Horizontal |  | **FAIL** |
| 120kHz | 432.11 | Vertical | - | RNDS-C-00517 V4.0 | 5 | PASS |
| Q-Peak | 432.47 | Vertical | - | - | 3 | **FAIL** |
| Q-Peak | 435.95 | Vertical | - | - | 5 | **FAIL** |
| Q-Peak | 432.56 | Vertical | - | - | 1 | **FAIL** |
| 1MHz | 237 | Vertical | 4 | RNDS-C-00517 V4.0 |  | **FAIL** |
| Peak | 243.75 | Vertical | 10 | - |  | **FAIL** |
| Peak | 240.75 | Vertical | 9 | - |  | **FAIL** |
| Peak | 243.25 | Vertical | 7 | - |  | **FAIL** |
| 9kHz | 1.162 | Vertical | - | RNDS-C-00517 V4.0 | 30 | PASS |
| GNSS | 1175.908 | Vertical | - | RNDS-C-00517 V4.0 | 5 | PASS |
| GNSS | 1599.87325 | Vertical | - | Horizontal | 4 | PASS |
| GNSS | 1175.90575 | Vertical | - | Horizontal | 3 | PASS |
| GNSS | 1175.90575 | Vertical | - | Horizontal | 1 | PASS |
| 120kHz | 432.56 | Vertical | - | RNDS-C-00517 V4.0 | 5 | PASS |
| Q-Peak | 432.68 | Vertical | - | - | 4 | **FAIL** |
| Q-Peak | 434.69 | Vertical | - | - | 4 | **FAIL** |
| Q-Peak | 432.29 | Vertical | - | - | 2 | **FAIL** |
| 1MHz | 238.25 | Vertical | 6 | RNDS-C-00517 V4.0 |  | **FAIL** |
| Peak | 244 | Vertical | 13 | - |  | **FAIL** |
| Peak | 237 | Vertical | 13 | - |  | **FAIL** |
| Peak | 244.5 | Vertical | 11 | - |  | **FAIL** |

"VotreNom" | 20/09/2025 | 2bdbeac262482322888ef9be8879a83e